Dips > Data Input > Grid Data > Data Columns

# Borehole Orientation Data Pairs

If orientation data was measured from the logging of core from a borehole, then the Traverse Type will be defined as BOREHOLE. For borehole traverses, the Orientation Columns must then contain the measurements of the "Alpha" and "Beta" angles, as defined below:

Alpha (entered in Orientation Column 1)

The minimum angle between the maximum dip vector of the plane of the discontinuity, and the core axis.

Beta (entered in Orientation Column 2)

The clockwise angle from the reference line to the direction of the maximum dip vector, looking along the direction of borehole advance.

See the figures below for illustration.

****************************************************************

IMPORTANT NOTE!!!
Also see the Borehole Traverse Orientation topic for ESSENTIAL INFORMATION concerning the orientation data required (orientations 1, 2 and 3) to set up a borehole logging traverse.

****************************************************************

If your data set was entirely recorded from borehole core logging, you will have to specify a traverse for each borehole, in the Traverse Information dialog, and set up the data accordingly.

ORIENTATION PARAMETERS FOR BOREHOLE DATA

DEFINITION OF ALPHA ANGLE

DEFINITION OF BETA ANGLE