Dips > Data Input > Traverses

# Traverse Orientation Format

By default, the orientation format of the data recorded on each traverse is the same as the Global Orientation Format.

However, the Traverse Orientation Format can be used to specify a different orientation format for any traverse. This is useful when combining data from different sources or when combining measurements of LINEAR features with measurements of PLANAR structures. Four different Traverse Orientation Formats may be used:

DIP/DIPDIRECTION

STRIKE(R)/DIP (right hand rule for strike)

STRIKE(L)/DIP (left hand rule for strike)

TREND/PLUNGE (use this for linear measurements)

NOTE: the Traverse Orientation Format is not applicable if the Traverse Type is BOREHOLE – it is only relevant for LINEAR, PLANAR or CLINORULE traverse types.