Dips > Data Input > Traverses

# Planar Traverse Orientation

If the Traverse Type is PLANAR, then the Orient 1 / Orient 2 values in the Traverse Information dialog are defined as follows:

The Plane in a PLANAR traverse is described by two orientation values, presented in the form which corresponds to the Traverse Orientation Format. The appropriate forms for Orient 1 / Orient 2 are:

00; 000 (DIP/DIPDIRECTION)

000; 00 (STRIKE/DIPR or STRIKE/DIPL)

000; 00 (TREND/PLUNGE of normal to the plane)